Contents List:

Application Form: – Attached

Amendment Record Sheet: Page 2

Product Description: Page 3

Visual Identification of Product: Page 3

Components Specification: Page 4, Foam attached

Test Reports: Attached

Declaration of Conformity: Page 5

Marking: Page 6

User Information: Page 7

Amendment Record Sheet:

Amendment: Date: Signature

Visor closure changed to 19684C 13/5/20 IJ

Visor closure changed to 19684D 28/5/20 IJ

Product Description: Visual identification of the product

A picture containing computer, table, desk, laptop

Description automatically generatedThe Staeger Face Visor incorporates two components, 240um recycled PET and a medically approved piece of Foam, size 150 length x 40mm width x 30mm depth. The Foam is not known to cause skin irritation when in contact with the wearer of the eye-protector.

A screenshot of text

Description automatically generated

Component Specification:

A screenshot of text

Description automatically generated

Declaration of Conformity

A screenshot of a cell phone

Description automatically generated

Marking: CE shall be placed on the product as well as the model designation. CE 728708, Staeger Face Visor.

User Information:

Staeger Face Visor produced by:

Staeger Clear Packaging, Unit 1 Swallowgate Business Park, Coventry CV6 4BL.

To protect against the ingress of Covid-19 virus into the face.

The protective Faceshield/Visor is manufactured for Covid-protection only. This filtering Faceshield/Visor is not a PPE device for general use and shall not be used for purposes other than protection against COVID-19.

The Staeger Face Visor is a single use product and should be disposed of at the end of the shift.

The Staeger Face Visor conforms to BSI’s PPE for Healthcare Professional 2020/403 /Eye protection.

The examining body was BSI, Kitemark Court, Davy Avenue Knowlhill, Milton Keynes, MK5 8PP, NB number 0086